Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM216	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	B. Murphy	Locality:
	Date Desc.:	13/03/92	Elevation:	220 metres
	Map Ref.:	Sheet No. : 8327   1:100000	Rainfall:	No Data
	Northing/Long.:	6086600 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	506700  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy2.23
	ASC Confidence:	Great Soil Group:	Yellow earth
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.02 m	Brown (7.5YR5/4-Moist); Light brown (7.5YR6/4-Dry); ; Fine sandy loam; Massive grade of 
	structure; Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-
	5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Field pH 5 (Raupach); 
	Common, very fine (0-1mm) roots; Common, fine (1-2mm) roots; Gradual change to - 
	A21	0.02 - 0.1 m	Brown (7.5YR5/4-Moist); Light brown (7.5YR6/4-Dry); ; Fine sandy loam; Massive grade of 
	structure; Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-
	5 per 100mm2) Fine (1-2mm) macropores, Dry; Very firm consistence; Field pH 4.5 (Raupach); 
	Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Gradual change to - 
	B1	0.1 - 0.28 m	Strong brown (7.5YR5/6-Moist); Reddish yellow (7.5YR6/6-Dry); ; Loam; Massive grade of 
	structure; Earthy fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-
	5 per 100mm2) Fine (1-2mm) macropores, Dry; Very firm consistence; Field pH 5.5 (Raupach); 
	Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Gradual change to - 
	B21	0.28 - 0.49 m	Yellowish red (5YR5/8-Moist); Reddish yellow (5YR6/8-Dry); ; Light clay; Moderate grade of 
	structure, 20-50 mm, Subangular blocky; 20-50 mm, Columnar; Rough-ped fabric; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Firm consistence; Common cutans, 10-50% of ped faces or walls coated, 
	faint; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Veins; Field pH 7 (Raupach); Few, very fine (0-1mm) 
	roots; Few, fine (1-2mm) roots; Gradual change to - 
	B31	0.49 - 0.77 m	Reddish yellow (7.5YR6/6-Moist); Reddish yellow (7.5YR6/8-Dry); Substrate influence, 20-50%
	 , Distinct; Light medium clay; Strong grade of structure, 20-50 mm, Subangular blocky; 20-50 
	mm, Columnar; Smooth-ped fabric; Dry; Weak consistence; Many cutans, >50% of ped faces or
	 walls coated, distinct; Very many (50 - 100 %), Ferromanganiferous, Medium (2 -6 mm), 
	Nodules; Very many (50 - 100 %), Ferromanganiferous, Medium (2 -6 mm), Veins; Field pH 8 
	(Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Gradual change to - 
	B23	0.77 - 0.9 m	Brownish yellow (10YR6/6-Moist); Brownish yellow (10YR6/6-Dry); Substrate influence, 10-
	20% , Distinct; Medium clay; Strong grade of structure, 20-50 mm, Subangular blocky; 100-200 
	mm, Prismatic; Smooth-ped fabric; Dry; Weak consistence; Many cutans, >50% of ped faces or 
	walls coated, distinct; Common (10 - 20 %), Ferromanganiferous, , ; Field pH 8 (Raupach); 
	Morphological Notes
	Observation Notes

	Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM216	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	YATE'S TRANSECT D                     
	Site Notes

	Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM216	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	SOIL STRUCTURE & MANAGEMENT             
	Project Code:	SSM	Site ID:	SSM216	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile