Project Name:	TS
	Project Code:	TS	Site ID:	C202	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	B.E. Butler	Locality:	Sullivans Terrace;Canberra 4 mile Military 17.1/35.9:
	Date Desc.:	01/03/55	Elevation:	No Data
	Map Ref.:	Rainfall:	635
	Northing/Long.:	Runoff:	No Data
	Easting/Lat.:	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn3
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark grey (2.5Y4/1-Moist); Olive grey (5Y5/2-Dry); ; Silty clay loam; Massive grade of structure;
	 2-10%, medium gravelly, 6-20mm, Sand, coarse fragments; , , , Concretions; Field pH 5.5 (pH 
	meter); Diffuse change to - 
	0.1 - 0.21 m	Black (2.5Y2/1-Moist); ; Silty medium clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Strong grade of structure, 50-100 mm, Prismatic; Moderately plastic; 0-2%, medium 
	gravelly, 6-20mm, Sand, coarse fragments; , , , Concretions; Field pH 6 (pH meter); Diffuse 
	change to - 
	0.21 - 0.33 m	Black (2.5Y2/1-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Subangular blocky; 
	Strong grade of structure, 50-100 mm, Prismatic; Moderately plastic; 0-2%, medium gravelly, 6-
	20mm, Sand, coarse fragments; , , , Concretions; Field pH 8 (pH meter); Diffuse change to - 
	0.33 - 0.43 m	Black (2.5Y2/1-Moist); ; Light clay (Heavy); Moderate grade of structure, 10-20 mm, Subangular
	 blocky; Strong grade of structure, 50-100 mm, Prismatic; Moderately plastic; 0-2%, medium 
	gravelly, 6-20mm, Sand, coarse fragments; , , , Concretions; Very few (0 - 2 %), Gypseous, , ; 
	Field pH 8.6 (pH meter); Sharp change to - 
	0.43 - 0.57 m	Black (2.5Y2/1-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular blocky; 
	Strong grade of structure, 20-50 mm, Prismatic; 0-2%, medium gravelly, 6-20mm, Sand, coarse 
	fragments; , , , Concretions; Few (2 - 10 %), Gypseous, , ; Field pH 8.8 (pH meter); 
	Morphological Notes
	Observation Notes
	LAYER 1-FINE MICA AND SAND;LAYER 2 NUMEROUS WORM CASTS:                                                                 
	Site Notes
	CANBERRA

	Project Name:	TS
	Project Code:	TS	Site ID:	C202	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.4H	 0.02B	 14.7K	 5	 0.64	 0.15	 8.2D
	0.1 - 0.21	7H	 0.017B	 19.4K	 7.2	 0.37	 0.18	 4.9D
	0.21 - 0.33	7.5H	 0.017B	 18.4K	 7.9	 0.38	 0.14	 3.3D
	0.33 - 0.43	8.2H	 0.039B
	0.43 - 0.57	8.4H	 0.044B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.029C	 0.227B	<1	 3C	 23	 42	 27
	0.1 - 0.21	 0.028C	 0.174B	 1C	 15	 44	 32
	0.21 - 0.33	 0.023C	 0.014B	 1C	 15	 44	 35
	0.33 - 0.43	 0.36C	 1C	 13	 42	 38
	0.43 - 0.57	 0.46C	 2	 2C	 13	 33	 44
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.21
	0.21 - 0.33
	0.33 - 0.43
	0.43 - 0.57

	Project Name:	TS
	Project Code:	TS	Site ID:	C202	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded