Project Name:	TS
	Project Code:	TS	Site ID:	C203	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	B.E. Butler	Locality:	Canberra Military Sheet 17.2/36.1:Banshaw Terrace:
	Date Desc.:	01/03/55	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	Runoff:	No Data
	Easting/Lat.:	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.33
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.13 m	Dark greyish brown (10YR4/2-Moist); Light brownish grey (10YR6/2-Dry); ; Loam (Heavy); 
	Moderate grade of structure, 5-10 mm, Subangular blocky; 10-20%, fine gravelly, 2-6mm, 
	Quartz, coarse fragments; Field pH 6 (pH meter); Diffuse change to - 
	A12	0.13 - 0.28 m	Dark greyish brown (10YR4/2-Moist); Light brownish grey (10YR6/2-Dry); ; Clay loam (Light); 
	Massive grade of structure; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6 
	(pH meter); Gradual change to - 
	A2	0.28 - 0.43 m	Olive yellow (2.5Y6/5-Moist); ; Sandy loam (Light); Massive grade of structure; Field pH 6.5 (pH 
	meter); Gradual change to - 
	B11	0.43 - 0.55 m	Brown (10YR5/3-Moist); ; Sandy light clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Strong grade of structure, 100-200 mm, Columnar; 10-20%, fine gravelly, 2-6mm, 
	Substrate material, coarse fragments; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), Nodules;
	 Field pH 7 (pH meter); Sharp change to - 
	B12	0.55 - 0.73 m	Light yellowish brown (10YR6/4-Moist); ; Sandy light clay (Heavy); Moderate grade of 
	structure, 20-50 mm, Angular blocky; Strong grade of structure, 100-200 mm, Columnar; 2-10%,
	 fine gravelly, 2-6mm, Substrate material, coarse fragments; Few (2 - 10 %), Ferruginous, 
	Medium (2 -6 mm), Nodules; Few (2 - 10 %), Calcareous, , ; Field pH 9 (pH meter); Gradual 
	C	0.78 - 0.88 m	Light yellowish brown (10YR6/4-Moist); ; Clay loam; Massive grade of structure; Many (20 - 50 
	%), Calcareous, , ; Field pH 9.5 (pH meter); Gradual change to - 
	Morphological Notes
	Observation Notes
	Site Notes
	CANBERRA

	Project Name:	TS
	Project Code:	TS	Site ID:	C203	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.3	6.3H	 0.012B	 5.7K	 1	 0.68	 0.04	 4.9D
	0.13 - 0.43	6.6H	 0.01B	 5.7K	 1.1	 0.45	 0.02	 3.1D
	0.28 - 0.58	7H	 0.008B	 3.8K	 1.8	 0.35	 0.02	 1.7D
	0.43 - 0.73	7.6H	 0.012B	 5.1K	 3.2	 1.3	 0.04	 1.6D
	0.55 - 0.85	8.7H	 0.053B
	0.78 - 1.08	9.3H	 0.051B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.3	 0.036C	 0.114B	 4	 28C	 33	 25	 11
	0.13 - 0.43	 0.029C	 0.071B	 6	 22C	 32	 31	 13
	0.28 - 0.58	 0.026C	 7	 27C	 33	 31	 7
	0.43 - 0.73	 6	 29C	 31	 14	 19
	0.55 - 0.85	 0.64C	 6	 26C	 31	 18	 19
	0.78 - 1.08	 9.3C	 8	 27C	 28	 16	 12
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.3
	0.13 - 0.43
	0.28 - 0.58
	0.43 - 0.73
	0.55 - 0.85
	0.78 - 1.08

	Project Name:	TS
	Project Code:	TS	Site ID:	C203	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded