Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD76	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	205 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6120434 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	536546  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	2 % 	Aspect:	135 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcareous Calcarosolic Redoxic Hydrosol Thick Non-gravelly	Principal Profile Form:	N/A
	 Clay-loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.13 m	Dark brown (7.5YR3/3-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Many (>5 
	per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) 
	macropores, Few (<1 per 100mm2) Medium (2-5mm) macropores, Dry; Weak consistence; 
	Common, medium (2-5mm) roots; Common, fine (1-2mm) roots; Many, very fine (0-1mm) roots; 
	Clear change to - 
	A12	0.13 - 0.48 m	Very dark brown (7.5YR2/2-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-
	2mm) macropores, Few (<1 per 100mm2) Medium (2-5mm) macropores, Dry; Weak 
	consistence; Many, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) 
	roots; Clear change to - 
	B21	0.48 - 0.72 m	Dark yellowish brown (10YR4/4-Moist); Mottles, 20-50% , Distinct; Light clay; Moderate grade 
	of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Many (>5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm 
	consistence; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules, weak, 
	segregations;Common (10 - 20 %), Manganiferous, , ; Common, very fine (0-1mm) roots; Few, 
	fine (1-2mm) roots; Clear change to - 
	B22	0.72 - 1 m	Strong brown (7.5YR5/6-Moist); Mottles, 20-50% , Distinct; Mottles, 10-20% , Distinct; Light 
	clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Few (<1 
	per 100mm2) Fine (1-2mm) macropores, Dry; Strong consistence; 2-10%, fine gravelly, 2-6mm, 
	subrounded, dispersed, coarse fragments; Common (10 - 20 %), Calcareous, Fine (0 - 2 mm), 
	Root linings, weak, segregations;Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; 
	Clear change to - 
	B23	1 - 1.43 m	Yellowish brown (10YR5/4-Moist); Mottles, 20-50% , Distinct; Mottles, 10-20% , Distinct; Light 
	clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Strong consistence; Many (20 - 50 %), Calcareous, Medium (2 -6 mm), 
	Fragments, strong, segregations;Many (20 - 50 %), Calcareous, Coarse (6 - 20 mm), 
	Fragments, strong, segregations;Clear change to - 
	B3	1.43 - 2 m	Yellowish brown (10YR5/4-Moist); Mottles, 20-50% , Distinct; Mottles, 10-20% , Distinct; Light 
	clay; Strong grade of structure, 5-10 mm, Subangular blocky; Common (1-5 per 100mm2) Very 
	fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Very firm 
	consistence; Many (20 - 50 %), Calcareous, Medium (2 -6 mm), Fragments, strong, 

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD76	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Observation Notes
	Site Notes
	Morphological Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD76	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	6.05A	0.116A	8.5J	1.8	1.7	0.03	12.8I	0.23
	0.13 - 0.48	6.32A	0.097A	10.1J	2.4	0.93	0.05	14I	0.36
	0.48 - 0.72	7.75A	0.834A	19.2J	3	1.6	0.07	15.5I	0.45
	0.72 - 1	8.12A	0.54A	21.4J	2.6	1	0.03	9.8I	0.31
	1 - 1.43	8.21A	0.976A	26J	10.5	1.2	0.34	13.5I	2.52
	1.43 - 2	8.17A	0.431A	18.7J	3.8	0.9	0.1	11.5I	0.87
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	2.29C	32.5I	20.6	46.9
	0.13 - 0.48	0.8C	36.1I	17.8	46.1
	0.48 - 0.72	0.33C	48.1I	12.9	39
	0.72 - 1	1.04C	34.7I	16.3	49
	1 - 1.43	1.96C	53.5I	18.8	27.7
	1.43 - 2	0.58C	34.4I	13.8	51.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.48
	0.48 - 0.72
	0.72 - 1
	1 - 1.43
	1.43 - 2

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD76	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded