Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD8	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	McKane, Dermot	Locality:
	Date Desc.:	15/07/93	Elevation:	246 metres
	Map Ref.:	Sheet No. : 8327   DGPS	Rainfall:	No Data
	Northing/Long.:	6123790 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	534290  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	5 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Red Chromosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Brown (7.5YR4/4-Moist); ; Coarse sandy loam; Massive grade of structure; Earthy fabric; Few 
	(<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very firm consistence; 2-10%, fine 
	gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Field pH 7 (pH meter); 
	Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	B2	0.15 - 0.6 m	Red (2.5YR4/6-Moist); ; Light clay; Moderate grade of structure, 2-5 mm, Subangular blocky; 
	Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Firm 
	consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; 0-2%, fine 
	gravelly, 2-6mm, subrounded, coarse fragments; Field pH 6.5 (pH meter); Few, very fine (0-
	1mm) roots; Gradual, Smooth change to - 
	BC	0.6 - 1 m	Strong brown (7.5YR5/8-Moist); Mottles, 2-10% , Distinct; Light medium clay; Moderate grade of
	 structure, 2-5 mm, Platy; Smooth-ped fabric; Dry; Firm consistence; 0-2%, fine gravelly, 2-6mm,
	 subangular, Quartz, coarse fragments; Very few (0 - 2 %), Ferromanganiferous, , ; Field pH 6 
	(pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD8	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	5.5A	0.056A	1.8J	1.8	1	0.11	5.9I	1.86
	0.15 - 0.6	6.86A	0.04A	5.9J	5.8	1.2	0.15	11.7I	1.28
	0.6 - 1	7.43A	0.041A	4.5J	4.5	0.54	0.08	9.2I	0.87
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	1.16C	25.5I	8.6	65.9
	0.15 - 0.6	0.48C	55.8I	9.1	35.1
	0.6 - 1	0.2C	45.3I	10.2	44.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.6
	0.6 - 1

	Project Name:	BRUCEDALE/LADYSMITH/GRIGGWARD - Soil Landscape Modelling
	Project Code:	Wagga_SLM	Site ID:	BD8	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15L1	Base saturation percentage (BSP)
	15N1	Exchangeable sodium percentage (ESP)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_S	Sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded