Agency Code: 501 Project Code: DAN Site Code: 0116
Described by: Ted (E.A.) Griffin Date: 29/05/1995

Observation type: auger boring Category: brief description

Location: MGA94 Zone: 50  375725 mE  6602852 mN 
Location notes: Kayanaba
Site notes: 
Disturbance: Complete clearing; never cultivated.

Landform
Landform pattern: peneplain	Slope:  2 %
Relief/modal slope: undulating low hills
Landform element: hillslope
Morphological type: upper slope
Pattern Relief:  peneplain

Surface and Hydrological Properties
Rock outcrop: 0 %  
Surface coarse fragments: no stones and boulder sized
Physical properties: soft; 

Vegetation
Notes: Euc calophylla

Species List
Eucalyptus calophylla

Land use
Site: Grazing (grazing of vegetation planted by man). Surrounds: Grazing (grazing of vegetation planted by man).

Current Classification
WA Soil Group: (1999) Brown deep sand
Soil Series: Sdb-r>150 (provisional)
Map Unit: 222Da_2a

Soil Profile Description

Horizon | Depth (cm) | Description
A1eh | 0-10 | Light brownish grey (10YR 6/2 moist) humic medium sand with <2% clay; strongly water repellent.
A31 | 10-20 | Dark greyish brown (10YR 4/2 moist) medium sand with <2% clay; strongly water repellent.
A32 | 20-150 | Strong brown (7.5YR 4/6 moist) medium sand with <2% clay.
A33 | 150-160 | Yellowish red (5YR 4/6 moist) medium sand with <2% clay.
B2 | 160-200+ | Strong brown (7.5YR 5/6 moist) sand with 2-4% clay.