Agency Code: 501 Project Code: WBW Site Code: 0708
Described by: Peter Tille Date: 22/01/1992

Observation type: auger boring Category: 

Location: MGA94 Zone: 50  442796 mE  6281569 mN Map sheet:  Bridgetown 100K
Location notes: Boupbrook Rd. North, Evans
Site notes: bleached sand over gravel (BSG)
Disturbance: Complete clearing; never cultivated.

Landform
Landform pattern:	Slope:  0 %
Relief/modal slope:
Landform element:
Morphological type: flat
Pattern Relief: 

Surface and Hydrological Properties
Rock outcrop:   
Surface coarse fragments: 
Physical properties: firm; 

Vegetation
Notes: Open woodlands, marri, jarrah, B.grandis

Current Classification
WA Soil Group: (1999) Grey deep sandy duplex
Australian Soil Classification: (2002) Bleached-Ferric Mesotrophic Grey Chromosol
ASC confidence: moderate
Soil Series: Eulanda 1
Map Unit: 255DpWGw

Soil Profile Description

Horizon	Depth (cm)	Description	
A1	0-10	Black (7.5YR 2/0 dry) sand; sandy fabric; single grain structure; subangular coarse fragments; pH 5; clear boundary.	
A21	10-35	Light grey (10YR 7/1 dry) sand; very few faint mottles; sandy fabric; single grain, and  massive structure; pH 6.5; clear boundary.	
A22	35-55	Pale brown (10YR 6/3 dry) sand; many subrounded quartz medium gravel sized coarse fragments and  rounded ferruginous gravel coarse fragments; pH 6.5; clear boundary.	
B2	55-75+	Very pale brown (10YR 8/3 dry) light clay; many distinct mottles; many subangular ferruginous gravel fine gravel sized coarse fragments and  subrounded coarse fragments; pH 7.