Agency Code: 501 Project Code: MB Site Code: 0141
Described by: Martin Wells Date: 06/09/1983

Observation type: auger boring Category: 

Location: MGA94 Zone: 50  371698 mE  6379583 mN Map sheet:  Pinjarra 100K
Location notes: 
Site notes: Marginal pleistocene flat
Disturbance: Limited clearing.

Landform
Landform pattern:	Slope:  2 %
Relief/modal slope:
Landform element: plain
Morphological type: flat
Pattern Relief: 	Microrelief: 1 m

Surface and Hydrological Properties
Rock outcrop:   
Surface coarse fragments: 
Physical properties: loose; ; shallow soil

Geology/parent material
Soil parent material: limestone

Current Classification
WA Soil Group: (1999) Yellow/brown shallow sand
Soil Series: 26b
Map Unit: 211Va__V6

Other Classifications
Northcote PPF: Uc5.11+

Soil Profile Description

Horizon | Depth (cm) | Description
A | 0-12 | Dark brown (10YR 3/3 moist) loamy sand; loose moist consistence; earthy fabric; massive structure; pH 7; abrupt boundary.
B | 12-20 | Brownish yellow (10YR 6/6 moist) sand; loose moist consistence; sandy fabric; single grain structure; pH 6.5; abrupt boundary.
C | 20-25+ |